Hunter Industries has provided all construction details in an Adobe PDF format for users 
who do not have cad.  A PDF reader can be downloaded to view and print these files. All these details
are drawn to scale with the scale of the detail listed at the bottom of the detail.

There are PDF Files for each type of construction technique. In order to supply the end user a detail that 
fits most common construction practices in their region, we have supplied 4 different details for 4 different 
construction practices for the Spray Heads.

The following is a legend for each PROS-04-PRS40 Spray Head Model. 
A and B denote a bubble and leader callout respectively.

PROS-04-PRS40-1A = PROS-04-PRS40 with 1/2" Sch 80 Nipples and 3 Sch 40 Street Ells
PROS-04-PRS40-1B
PROS-04-PRS40-2A = PROS-04-PRS40 with 1/2" Sch 80 Nipple and 3 MARLEX 90 Elbows
PROS-04-PRS40-2B
PROS-04-PRS40-3A = PROS-04-PRS40 with Hunter Swing Joint Model SJ-5XX-X
PROS-04-PRS40-3B
PROS-04-PRS40-4A = PROS-04-PRS40 with Hunter "Pro Flex" Tubing, 2-Hunter HSBE-050 Elbows and one MARLEX 90 Elbow
PROS-04-PRS40-4B

