Hunter Industries has provided all construction details in an Adobe PDF format for users 
who do not have cad.  A PDF reader can be downloaded to view and print these files. All these details
are drawn to scale with the scale of the detail listed at the bottom of the detail.

There are PDF Files for each type of construction technique. In order to supply the end user a detail that 
fits most common construction practices in their region; we have supplied 2 different details for 2 different 
construction practices for the IBV-101G Valve.

The following is a legend for each IBV-101G Valve
A and B denote a bubble and leader callout respectively.

IBV-101G-1A =  IBV-101G With Sch 80 Slip Unions
IBV-101G-1B
IBV-101G-2A =  IBV-101G With Sch 80 TOE Nipples
IBV-101G-2B

There are also details with IS in the file name that use and Isolation valve upstream of the IBV.
